**DEVELOP THE PYTHON CODE**

|  |  |
| --- | --- |
| **Date** | 16th November 2022 |
| **Team ID** | PNT2022TMID45387 |
| **Project Name** | Gas Leakage Monitoring and Alerting  System |
| **Maximum Mark** | 4 marks |

**TEAM LEADER: ABDUL AZIZ M**

**TEAM MEMBER 1: KARTHICK PANDIYAN R**

**TEAM MEMBER 2: JEGAN J**

**TEAM MEMBER 3: AYYANAR S**

**PYTHON CODE:**

import time

import sys

import ibmiotf.application

import ibmiotf.device

import random

#Provide your IBM Watson Device Credentials

organization = "5py6q9"

deviceType = "Weather\_now"

deviceId = "Weather1234"

authMethod = "token"

authToken = "XeJFia7\_@@t9@@eq\_?"

# Initialize GPIO

def myCommandCallback(cmd):

print("Command received: %s" % cmd.data['command'])

status=cmd.data['command']

if status=="lighton":

print ("led is on")

elif status == "lightoff":

print ("led is off")

else :

print ("please send proper command")

try:

deviceOptions = {"org": organization, "type": deviceType, "id": deviceId, "auth-method": authMethod, "auth-token": authToken}

deviceCli = ibmiotf.device.Client(deviceOptions)

#..............................................

except Exception as e:

print("Caught exception connecting device: %s" % str(e))

sys.exit()

# Connect and send a datapoint "hello" with value "world" into the cloud as an event of type "greeting" 10 times

deviceCli.connect()

while True:

#Get Sensor Data from DHT11

temp=random.randint(90,110)

Humid=random.randint(60,100)

data = { 'temp' : temp, 'Humid': Humid }

#print data

def myOnPublishCallback():

print ("Published Temperature = %s C" % temp, "Humidity = %s %%" % Humid, "to IBM Watson")

success = deviceCli.publishEvent("IoTSensor", "json", data, qos=0, on\_publish=myOnPublishCallback)

if not success:

print("Not connected to IoTF")

time.sleep(10)

deviceCli.commandCallback = myCommandCallback

# Disconnect the device and application from the cloud

deviceCli.disconnect()